1080P Sony Exmor Sensor (TVI/AHD/CVI/1200tvl) 2.8-12mm Manual Zoom HD Security Camera, Honic 2MP Varifocal IR CCTV Cameras, Outdoor Waterproof Day Night Vision Analog Camera for Video Surveillance

CRISP IMAGE: 1/2.9-inch Sony Exmor sensor & megapixel Lens for crystal clear image. Low Illumination, D-WDR, AGC, AWB, 3DNR and multiple OSD adjustments for optimal picture quality in any given lighting condition.

ENHANCED NIGHT VISION: Latest tech anti-reflection black film panel, IR filter and upgraded Led with 100-130 feet Long range IR for superior image at night.

GREAT LOW LIGHT IMAGE: SONY Exmor image sensor with NIR and LOW ILLUMINATION technology applied, it performs great image with little ambient light.

4 MODES OUTPUT: 2 Megapixel HD-TVI, 2.0MP HDCVI, 2.0 MP AHD and 1200 tvl wired BNC video output.

PEACE OF MIND WARRANTY: 60 DAY money back guarantee, 24 MONTH warranty and friendly, easy-to-reach support; Power supply (Need DC 12V 2A), coaxial video cable and DVR are NOT INCLUDED but REQUIRED